GLYTCH PANEL ARTWORK PACKAGE v0.1

Please use your Yisonprinting double-door / gatefold rigid box template/dieline.

We are providing artwork images per panel for each flavor. Please place these artwork files onto your official dieline/template and prepare final production AI/PDF proof files.

IMPORTANT:
- These are panel artwork direction files, not the final dieline placement.
- Please add 3mm bleed where needed.
- Please keep all text/logos inside safe margins away from folds/cuts.
- Please prepare final print files with separate layers:
  1. DIELINE / cut / fold lines
  2. CMYK ARTWORK
  3. SPOT UV mask
  4. FOIL mask
  5. EMBOSS / DEBOSS mask
- Please send a digital proof before physical sample production.

BOX CONTENTS:
- HDPE powder tub: approx 90mm diameter x 85mm tall, 300g fill.
- Collectible card pack: finished foil pack not final yet; please allow around 70 x 100 x 8mm and advise proper clearance.
- Preferred insert: black EVA foam tray.

PANEL FILES PER FLAVOR:
01_OUTSIDE_FRONT_CLOSED_200x105mm.png
- Closed box hero/front artwork. It is designed as a 200 x 105mm full face and can be split across the two front doors if needed.

02_INSIDE_DOORS_SPREAD_200x105mm.png
- Artwork for the inside door spread when the box opens.

03_TRAY_BASE_ART_200x130mm.png
- Interior tray/base artwork. Shows tub well, card pack pocket, and app/QR placement.

04_LEFT_SIDE_PANEL_130x105mm.png
- Left side panel artwork.

05_RIGHT_SIDE_PANEL_130x105mm.png
- Right side panel artwork.

06_LEGAL_BACK_PANEL_130x105mm.png
- Draft legal/back panel. UPC and some regulatory copy are placeholders until final review.

FINISH REQUESTS:
- Base: matte black lamination.
- Logo area: foil + emboss/deboss.
- Character art: spot UV.
- Glitch pattern/energy lines: spot UV.
- Interior: flavor-color flood print.

LEGAL / PLACEHOLDERS:
- UPC barcode is placeholder. We will provide final UPC later.
- QR is placeholder. We will provide final app QR later.
- Supplement facts / ingredients are draft placement copy and must be checked before final print.
- Do not print until final proof is approved.
